* Making should be done for Vias.
* Differential Impedance is fine.
* Lengths are fine.
* Probe connector pin out is fine. Checked by placing.